;===========================================================================
; 
; Windows 2000, 98/ME NDIS driver INF for Libertas 802.11b/g Wireless
; Copyright (C) 2004 Marvell Semiconductor, Inc.
;
;=========================================================================== 
 
 
[Version] 
Signature = "$CHICAGO$" 
Compatible  = 1
Class=Net
ClassGUID={4D36E972-E325-11CE-BFC1-08002BE10318} 
Provider=%MRVL% 
;CatalogFile=Mrv8000c.cat
MillenniumPreferred = .ME
DriverVer=02/22/2005,3.1.1.7

;===========================================================================
; Source Media Information Sections
;===========================================================================
[SourceDisksNames]
1 = "Marvell installation disk 1",,,

[SourceDisksFiles]
; On Marvell installation disk 1 
Mrv8000c.sys =1 

[DestinationDirs]
W8335PCI.2K.CopyFiles  = 12 
W8335PCI.W9x.CopyFiles = 11
DefaultDestDirs        = 11

[Manufacturer] 
%MRVL%=MarvellDevices

[MarvellDevices]
%W8335PCI.DeviceDesc% = W8335PCI.ndi, PCI\VEN_11AB&DEV_1FAA
%W8335PXPCI.DeviceDesc% = W8335PXPCI.ndi, PCI\VEN_11AB&DEV_1FAB

;===========================================================================
; ControlFlags section
;===========================================================================
[ControlFlags]
ExcludeFromSelect = *

;***************************************************************************
;***************************************************************************
;**         
;**          Win 2K DDInstall section
;**          
;***************************************************************************
;***************************************************************************

[W8335PCI.ndi.NT]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is PCI or CardBus
BusType         = 5 
AddReg          = W8335PCI.reg, W8335PCI2K.reg
CopyFiles       = W8335PCI.2K.CopyFiles 

;===========================================================================
; W8335 PCI Win2K registers
;===========================================================================
[W8335PCI2K.reg]
HKR, Ndi,            Service,    0, "W8335PCI"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"


[W8335PCI.2K.CopyFiles]
Mrv8000c.sys,,,2 



[W8335PCI.ndi.NT.Services]
AddService = W8335PCI, 2, W8335PCI2K.Service, Common.EventLog

[W8335PCI2K.Service]
DisplayName    = %W8335PCI2K.Service.DispName%
ServiceType    = 1 ;%SERVICE_KERNEL_DRIVER%
StartType      = 3 ;%SERVICE_DEMAND_START%
ErrorControl   = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\Mrv8000c.sys
LoadOrderGroup = NDIS

[Common.EventLog]
AddReg = Common.AddEventLog.reg

[Common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


;***************************************************************************
;***************************************************************************
;**         
;**          Win9X DDInstall section
;**          
;***************************************************************************
;***************************************************************************

[W8335PCI.ndi]
;Windows 98 doesn't recognize DriverVer in the [Version] section
;so include it here

DriverVer=02/22/2005,3.1.1.7
AddReg   = W8335PCI.reg, W8335PCI.devID.reg, W8335PCI.W9x.reg
DeviceID = "PCI\VEN_11AB&DEV_1FAA"
CopyFiles = W8335PCI.W9x.CopyFiles


[W8335PXPCI.ndi]
;Windows 98 doesn't recognize DriverVer in the [Version] section
;so include it here

DriverVer=02/22/2005,3.1.1.7
AddReg   = W8335PCI.reg, W8335PXPCI.devID.reg, W8335PCI.W9x.reg
DeviceID = "PCI\VEN_11AB&DEV_1FAB"
CopyFiles = W8335PCI.W9x.CopyFiles


[W8335PCI.W9x.CopyFiles]
Mrv8000c.sys,,,2


;===========================================================================
; Win9x device ID registry section
;===========================================================================
[W8335PCI.devID.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_11AB&DEV_1FAA"

[W8335PXPCI.devID.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_11AB&DEV_1FAB"

;===========================================================================
; W8335 PCI Win9x
;===========================================================================
[W8335PCI.W9x.reg]
HKR, , DevLoader,, *ndis,*ntkern
HKR, , DeviceVxDs,, Mrv8000c.sys

HKR, , EnumPropPages,0, "netdi.dll,EnumPropPages"

; Win98 can use NDIS 5 (NOT applied on Win 95)
HKR, Ndi\Interfaces,DefUpper,   0, "ndis3,ndis4,ndis5"
HKR, Ndi\Interfaces,DefLower,   0, "ethernet"
HKR, Ndi\Interfaces,UpperRange, 0, "ndis3,ndis4,ndis5"
HKR, Ndi\Interfaces,LowerRange, 0, "ethernet"

HKR, NDIS, LogDriverName,    0, "W8335PCI"
HKR, NDIS, MajorNdisVersion, 1, 05
HKR, NDIS, MinorNdisVersion, 1, 00

HKR, Ndi\Install, ndis5, 0, "W8335PCI.Install"
HKR, Ndi\Install, ndis4, 0, "W8335PCI.Install"


;===========================================================================
; W8335 PCI common, MIB can be defined here
;===========================================================================
[W8335PCI.reg]
HKR, Ndi\params\FragThsd,  ParamDesc,0 , "%FragThsd%"
HKR, Ndi\params\FragThsd,  default, 0 , "2346"
HKR, Ndi\params\FragThsd,  min, 0 , "256"
HKR, Ndi\params\FragThsd,  max, 0 , "2346"
HKR, Ndi\params\FragThsd,  step, 0 , "1"
HKR, Ndi\params\FragThsd,  Base, 0 , "10"
HKR, Ndi\params\FragThsd,  type, 0 ,"dword"

HKR, Ndi\params\RTSThsd,  ParamDesc, 0, "%RTSThsd%"
HKR, Ndi\params\RTSThsd,  default, 0, "2346"
HKR, Ndi\params\RTSThsd,  min, 0, "0"
HKR, Ndi\params\RTSThsd,  max, 0, "2346"
HKR, Ndi\params\RTSThsd,  step, 0, "1"
HKR, Ndi\params\RTSThsd,  Base, 0, "10"
HKR, Ndi\params\RTSThsd,  type, 0, "dword"

HKR, Ndi\params\PowerMode,ParamDesc,,"%PowerMode%"
HKR, Ndi\params\PowerMode,default,,"0"
HKR, Ndi\params\PowerMode,type,,enum
HKR, Ndi\params\PowerMode\enum,"0",,"CAM-Constantly Awake Mode"
HKR, Ndi\params\PowerMode\enum,"1",,"MaxPSP-Max Power Savings"
;HKR, Ndi\params\PowerMode\enum,"2",,"FastPSP-Fast Power Savings"

HKR, Ndi\params\Preamble,ParamDesc,,"%PreambleStr%"
HKR, Ndi\params\Preamble,default,,"3"
HKR, Ndi\params\Preamble,type,,enum 
HKR, Ndi\params\Preamble\enum,"1",,"Auto"
HKR, Ndi\params\Preamble\enum,"2",,"Short Preamble" 
HKR, Ndi\params\Preamble\enum,"3",,"Long Preamble"

HKR, Ndi\params\AdhocGMode,ParamDesc,,"%AdhocGMode%"
HKR, Ndi\params\AdhocGMode,default,,"1"
HKR, Ndi\params\AdhocGMode,type,,enum
HKR, Ndi\params\AdhocGMode\enum,"0",,"Adhoc G Mode"
HKR, Ndi\params\AdhocGMode\enum,"1",,"Adhoc B Mode only" 

HKR, Ndi\params\DesiredSSID,ParamDesc,,"%SSID%"
HKR, Ndi\params\DesiredSSID,default,,"MarvellAP3x"
HKR, Ndi\params\DesiredSSID,type,,"edit" 
HKR, Ndi\params\DesiredSSID,LimitText,,"32"
HKR, Ndi\params\DesiredSSID,UpperCase,,"0" 
HKR, Ndi\params\DesiredSSID,Optional,,"0" 

HKR, Ndi\xparams\AuthMode,ParamDesc,,"%AuthMode%"
HKR, Ndi\xparams\AuthMode,default,,"0"
HKR, Ndi\xparams\AuthMode,type,,enum
HKR, Ndi\xparams\AuthMode\enum,"0",,"Open"
HKR, Ndi\xparams\AuthMode\enum,"1",,"Shared"

HKR, Ndi\xparams\NetworkMode,ParamDesc,,"%NetworkMode%"
HKR, Ndi\xparams\NetworkMode,default,,"1"
HKR, Ndi\xparams\NetworkMode,type,,enum
HKR, Ndi\xparams\NetworkMode\enum,"0",,"Ad Hoc"
HKR, Ndi\xparams\NetworkMode\enum,"1",,"Infrastructure"

;HKR, Ndi\xparams\Wireless,ParamDesc,,"%WirelessM%"
;HKR, Ndi\xparams\Wireless,default,,"0"
;HKR, Ndi\xparams\Wireless,type,,enum
;HKR, Ndi\xparams\Wireless\enum,"0",,"Auto"
;HKR, Ndi\xparams\Wireless\enum,"1",,"B rates only"
 

HKR, Ndi\xparams\Channel,  ParamDesc,0 , "%Channel%"
HKR, Ndi\xparams\Channel,  default, 0 , "1"
HKR, Ndi\xparams\Channel,  min, 0 , "0"
HKR, Ndi\xparams\Channel,  max, 0 , "14"
HKR, Ndi\xparams\Channel,  step, 0 , "1"
HKR, Ndi\xparams\Channel,  Base, 0 , "16"
HKR, Ndi\xparams\Channel,  type, 0 ,"dword"

HKR, Ndi\xparams\TxAntenna,  ParamDesc,0 , "%TxAntennaStr%"
HKR, Ndi\xparams\TxAntenna,  default, 0 , "2"
HKR, Ndi\xparams\TxAntenna,  min, 0 , "1"
HKR, Ndi\xparams\TxAntenna,  max, 0 , "ffff"
HKR, Ndi\xparams\TxAntenna,  step, 0 , "1"
HKR, Ndi\xparams\TxAntenna,  Base, 0 , "16"
HKR, Ndi\xparams\TxAntenna,  type, 0 ,"dword"

HKR, Ndi\xparams\RxAntenna,  ParamDesc,0 , "%RxAntennaStr%"
HKR, Ndi\xparams\RxAntenna,  default, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna,  min, 0 , "1"
HKR, Ndi\xparams\RxAntenna,  max, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna,  step, 0 , "1"
HKR, Ndi\xparams\RxAntenna,  Base, 0 , "16"
HKR, Ndi\xparams\RxAntenna,  type, 0 ,"dword"

;
; LED Control
;
HKR,, LED0PowerOn, 2,"30001"
HKR,, LED1PowerOn, 2,"fe0101"
HKR,, LED0PowerOff, 2,"fe0000"
HKR,, LED1PowerOff, 2,"fe0100"
HKR,, LED0Scan, 2,"ff0002"
HKR,, LED1Scan, 2,"40102"
HKR,, LED0Associated, 2,"ff0005"
HKR,, LED1Associated, 2,"fe0105"
HKR,, LED0Joined, 2,"ff0006"
HKR,, LED1Joined, 2,"ff0106"
HKR,, LED0Started, 2,"ff0007"
HKR,, LED1Started, 2,"ff0107"
HKR,, LED0Tx, 2,"ff0008"
HKR,, LED1Tx, 2,"30108"
HKR,, LED0Rx, 2,"ff0009"
HKR,, LED1Rx, 2,"30109"
HKR,, LED0TxHigh, 2,"ff000c"
HKR,, LED1TxHigh, 2,"2010c"
HKR,, LED0RxHigh, 2,"ff000d"
HKR,, LED1RxHigh, 2,"2010d"

HKR,, LEDOffAfterRadioOff, 2, "1" 

HKR, Ndi\xparams\DataRate,ParamDesc,,"%DataRate%"
HKR, Ndi\xparams\DataRate,default,,"FF"
HKR, Ndi\xparams\DataRate,type,,enum
HKR, Ndi\xparams\DataRate\enum,"FF",,"Auto"
HKR, Ndi\xparams\DataRate\enum,"2",,"1 Mbps"
HKR, Ndi\xparams\DataRate\enum,"4",,"2 Mbps"
HKR, Ndi\xparams\DataRate\enum,"b",,"5.5 Mbps"
HKR, Ndi\xparams\DataRate\enum,"16",,"11 Mbps"
;HKR, Ndi\xparams\DataRate\enum,"2C",,"22 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"C",,"6 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"12",,"9 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"18",,"12 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"24",,"18 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"30",,"24 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"48",,"36 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"60",,"48 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"6C",,"54 Mbps"

HKR, Ndi\xparams\WepStatus,ParamDesc,,"%WepStatus%"
HKR, Ndi\xparams\WepStatus,default,,"1"
HKR, Ndi\xparams\WepStatus,type,,enum
HKR, Ndi\xparams\WepStatus\enum,"0",,"Enabled"
HKR, Ndi\xparams\WepStatus\enum,"1",,"Disabled"


HKR,, TxWepKey, 2, "" 
HKR,, WepKey1, 2, "" 
HKR,, WepKey2, 2, "" 
HKR,, WepKey3, 2, "" 
HKR,, WepKey4, 2, "" 

HKR,, DriverVer, 2, "3.1.1.7"
HKR,, DriverRel, 2, "02/22/2005"

;===========================================================================
; Strings section
;===========================================================================
[Strings]
MRVL = "AirLive"

TxAntennaStr = "Tx Antenna Select"
RxAntennaStr = "Rx Antenna Select" 
Channel = "Channel"
FragThsd = "Fragamentation Threshold"
DataRate = "Data Rate"
RTSThsd = "RTS Threshold"
AuthMode = "Authentication Mode"
;WirelessM = "Wireless Mode"
NetworkMode = "Operation Mode"
WepStatus = "WEP Status"
SSID = "SSID"
PreambleStr = "Preamble Select"
PowerMode = "Power Save Mode"
AdhocGMode = "Adhoc Mode"

LED0PowerOnStr    = "LED 0 Power On"
LED0PowerOffStr   = "LED 0 Power Off"
LED0ScanStr       = "LED 0 Site Survey"
LED0AssociatedStr = "LED 0 Associated"
LED0JoinedStr     = "LED 0 IBSS Joined"
LED0StartedStr    = "LED 0 IBSS Started"
LED0TxStr         = "LED 0 Tx"
LED0RxStr         = "LED 0 Rx"
LED0TxHighStr     = "LED 0 Tx High Traffic"
LED0RxHighStr     = "LED 0 Rx High Traffic"

LED1PowerOnStr    = "LED 1 Power On"
LED1PowerOffStr   = "LED 1 Power Off"
LED1ScanStr       = "LED 1 Site Survey"
LED1AssociatedStr = "LED 1 Associated"
LED1JoinedStr     = "LED 1 IBSS Joined"
LED1StartedStr    = "LED 1 IBSS Started"
LED1TxStr         = "LED 1 Tx"
LED1RxStr         = "LED 1 Rx"
LED1TxHighStr     = "LED 1 Tx High Traffic"
LED1RxHighStr     = "LED 1 Rx High Traffic"

W8335PCI.DeviceDesc	= "WL-5460PCM/PCI 802.11g Wireless LAN Card"
W8335PXPCI.DeviceDesc	= "WL-5460PCM/PCI 802.11g Wireless LAN Card"
W8335PCI2K.Service.DispName = "WL-5460PCM/PCI 802.11g Wireless LAN Card"




 
 
 
 
 
