**V6.B.2.7821**

|  |  |
| --- | --- |
| **Date** | 2012/01/19 |
| **Brand** | Airlive |
| **Model** | All |
| **Improved Features** |  |
|  | 1. Show warning message while viewer exceed maximum number. |
|  | 2. Open power frequency interface in IP-200PHD,IP-200PHD-24/24B,WN-200HD. |
|  | 3. Add AAC codec. |
|  |  |
|  |  |
| **Fixed Bugs** |  |
|  | 1. Can't set '%' at osd string. |
|  | 2. Streaming stop working while upload wrong file in firmware upgrade procedure. |
|  | 3. SD card auto mount cannot work while restart the IPCam. |
|  | 4. Improve av sync. |
|  | 5. Cannot set bitrate to maximum value. |
|  |  |
|  |  |
| **Notes** |  |
|  | Add new model: IP-200PD-24B IP-200PHD-24 |