;; Netrtuw.inf
;;
;; Realtek RTL8187 Wireless 802.11g 54Mbps USB 2.0 Network Adapter
;;
;; Copyright (C) 2008 Realtek Semiconductor Corp.
;;
;; this release is primarily for WHQL test.
;;

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider	= %Realtek%
CatalogFile.NT	= netrtuw.cat		;; for WHQL certified
DriverVer	= 06/13/2008,6.1313.0613.2008

[Manufacturer]
%Realtek% = Realtek,NTamd64.6.0

[ControlFlags]
ExcludeFromSelect = USB\VID_1B75&PID_8187&REV_0100

;;****************************************************************************
;; IDs for X86
;;****************************************************************************
[Realtek.NTx86.6.0]
%RTL8187.DeviceDesc% = RTL8187.ndi, USB\VID_1B75&PID_8187&REV_0100
%RTL8187.DeviceDesc% = RTL8187.ndi, USB\VID_13D1&PID_ABE6&REV_0100  
%RTL8187.DeviceDesc% = RTL8187.ndi, USB\VID_1371&PID_9401&REV_0100 
%RTL8187.DeviceDesc% = RTL8187.ndi, USB\VID_114B&PID_0150&REV_0100 
%RTL8187.DeviceDesc% = RTL8187.ndi, USB\VID_18E8&PID_6232&REV_0100 
%RTL8187.DeviceDesc% = RTL8187.ndi, USB\VID_0789&PID_010C&REV_0100

%RTL8187.DeviceDesc.Surecom% = RTL8187.ndi,USB\VID_0769&PID_11F2&REV_0100 
%RTL8187.DeviceDesc.Sitecom% = RTL8187.ndi,USB\VID_0DF6&PID_000D&REV_0100 

;;****************************************************************************
;; IDs for X64
;;****************************************************************************
[Realtek.NTamd64.6.0]
%RTL8187.DeviceDesc% = RTL8187.ndi, USB\VID_1B75&PID_8187&REV_0100
%RTL8187.DeviceDesc% = RTL8187.ndi, USB\VID_13D1&PID_ABE6&REV_0100  
%RTL8187.DeviceDesc% = RTL8187.ndi, USB\VID_1371&PID_9401&REV_0100 
%RTL8187.DeviceDesc% = RTL8187.ndi, USB\VID_114B&PID_0150&REV_0100 
%RTL8187.DeviceDesc% = RTL8187.ndi, USB\VID_18E8&PID_6232&REV_0100 
%RTL8187.DeviceDesc% = RTL8187.ndi, USB\VID_0789&PID_010C&REV_0100

%RTL8187.DeviceDesc.Surecom% = RTL8187.ndi,USB\VID_0769&PID_11F2&REV_0100 
%RTL8187.DeviceDesc.Sitecom% = RTL8187.ndi,USB\VID_0DF6&PID_000D&REV_0100 

;;****************************************************************************
;; Windows 2000/XP
;;****************************************************************************
[RTL8187.ndi.NT]
AddReg			= RTL8187.nt5.reg, RTL8187.common.reg, RTLWLAN.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTL8187.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8187.ndi.NT.Services]
AddService		= RTL8187, 2, RTL8187.nt5.Service, RTL8187.nt5.EventLog


;;****************************************************************************
;; Windows 2000/XP parameters
;;****************************************************************************
[RTL8187.nt5.reg]
HKR, Ndi\Interfaces,    UpperRange, 0, "ndis5,mdcwifi,wifipro"
HKR, Ndi\Interfaces,	LowerRange, 0, "wlan, ethernet"
HKR, Ndi,				Service,    0, "RTL8187"

[RTL8187.nt5.Service]
DisplayName    = %RTL8187.DeviceDesc.DispName%
ServiceType    = 1		; %SERVICE_KERNEL_DRIVER%
StartType      = 3		; %SERRVICE_DEMAND_START%
ErrorControl   = 1		; %SERRVICE_ERROR_NORMAL%
ServiceBinary  = %12%\RTL8187.sys
LoadOrderGroup = NDIS

[RTL8187.nt5.EventLog]
AddReg = RTL8187.nt5.AddEventLog.reg

[RTL8187.nt5.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7

;*******************************************************************************
; RTL8187 common paramters
;*******************************************************************************
[RTL8187.common.reg]
HKR,Ndi\params\LedCtrl,        ParamDesc,  0, %LED_CONTROL_STR%
HKR,Ndi\params\LedCtrl,        type,       0, "enum"
HKR,Ndi\params\LedCtrl,        default,    0, "1"
HKR,Ndi\params\LedCtrl\enum,   "0",        0, "Disable"
HKR,Ndi\params\LedCtrl\enum,   "1",        0, "Enable"
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,NDI\params\PowerSaveMode,      ParamDesc,  0, %POWER_SAVE_STR%
HKR,NDI\params\PowerSaveMode,      type,       0, "enum"
HKR,Ndi\params\PowerSaveMode,      default,    0, "0"
HKR,NDI\params\PowerSaveMode\enum, "0",        0, "CAM"
HKR,NDI\params\PowerSaveMode\enum, "1",        0, "MAX_PSP"
HKR,NDI\params\PowerSaveMode\enum, "2",        0, "Fast_PSP"
HKR,defaults,PowerSaveMode,0,"0"
HKR,,PowerSaveMode,0,"0"

HKR,Ndi\params\WiFi11bIbss,        ParamDesc,  0, %WIFI_IBSS_STR%
HKR,Ndi\params\WiFi11bIbss,        type,       0, "enum"
HKR,Ndi\params\WiFi11bIbss,        default,    0, "0"
HKR,Ndi\params\WiFi11bIbss\enum,   "0",        0, "Disable"
HKR,Ndi\params\WiFi11bIbss\enum,   "1",        0, "Enable"
HKR,defaults,WiFi11bIbss,0,"0"
HKR,,WiFi11bIbss,0,"0"

HKR,Ndi\params\bRateAdaptive,        ParamDesc,  0, %RATE_ADAPTIVE_STR%
HKR,Ndi\params\bRateAdaptive,        type,       0, "enum"
HKR,Ndi\params\bRateAdaptive,        default,    0, "1"
HKR,Ndi\params\bRateAdaptive\enum,   "0",        0, "Disable"
HKR,Ndi\params\bRateAdaptive\enum,   "1",        0, "Enable"
HKR,defaults,bRateAdaptive,0,"1"
HKR,,bRateAdaptive,0,"1"

; IC specific
HKR,,QoS,0,"0"
HKR,,CcxRm,0,"0"


;;----------------------------------------------------------------------------
;; Realtek WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTLWLAN.reg]
HKR,Ndi\params\SSID,   	      ParamDesc,  0, %SSID_STR%
HKR,Ndi\params\SSID,   	      type,       0, "edit"
HKR,Ndi\params\SSID,   	      default,    0, "ANY"
HKR,Ndi\params\SSID,   	      LimitText,  0, "32"
HKR,defaults,SSID,0,"ANY"
HKR,,SSID,0,"ANY"

HKR,Ndi\params\Channel,       ParamDesc,  0, %CHANNEL_STR%
HKR,Ndi\params\Channel,       type,       0, "int"
HKR,Ndi\params\Channel,       default,    0, "1"
HKR,Ndi\params\Channel,       Min,        0, "1"
HKR,Ndi\params\Channel,       Max,        0, "14"
HKR,Ndi\params\Channel,       Step,       0, "1"
HKR,Ndi\params\Channel,       Base,       0, "10"
HKR,defaults,Channel,0,"1"
HKR,,Channel,0,"1"

HKR,Ndi\params\NetworkType,        ParamDesc,  0, %NETWORK_TYPE_STR%
HKR,Ndi\params\NetworkType,        type,       0, "enum"
HKR,Ndi\params\NetworkType,        default,    0, "1"
HKR,Ndi\params\NetworkType\enum,   "0",        0, "Ad Hoc"
HKR,Ndi\params\NetworkType\enum,   "1",        0, "Infrastructure"
HKR,Ndi\params\NetworkType\enum,   "2",        0, "Auto select"
HKR,defaults,NetworkType,0,"1"
HKR,,NetworkType,0,"1"

HKR,Ndi\params\ChannelPlan, ParamDesc, 0, %CHANNEL_PLAN_STR%
HKR,Ndi\params\ChannelPlan, type, 0, "enum"
HKR,Ndi\params\ChannelPlan, default, 0, "15"
HKR,Ndi\params\ChannelPlan\enum, "0", 0, "FCC"
HKR,Ndi\params\ChannelPlan\enum, "1", 0, "IC"
HKR,Ndi\params\ChannelPlan\enum, "2", 0, "ETSI"
HKR,Ndi\params\ChannelPlan\enum, "3", 0, "Spain"
HKR,Ndi\params\ChannelPlan\enum, "4", 0, "France"
HKR,Ndi\params\ChannelPlan\enum, "5", 0, "MKK"
HKR,Ndi\params\ChannelPlan\enum, "6", 0, "MKK1"
HKR,Ndi\params\ChannelPlan\enum, "7", 0, "Israel"
HKR,Ndi\params\ChannelPlan\enum, "8", 0, "TELEC"
HKR,Ndi\params\ChannelPlan\enum, "15", 0, "DOMAIN_FROM_EEPROM"
HKR,defaults,ChannelPlan, 0, "15"
HKR,,ChannelPlan, 0, "15"

; Wireless Mode, 2006.11.30, by shien chang.
HKR,Ndi\params\WirelessMode, ParamDesc, 0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, type, 0, "enum"
HKR,Ndi\params\WirelessMode, default, 0, "8"
;HKR,Ndi\params\WirelessMode\enum, "1", 0, "IEEE 802.11a"
HKR,Ndi\params\WirelessMode\enum, "2", 0, "IEEE 802.11b"
HKR,Ndi\params\WirelessMode\enum, "4", 0, "IEEE 802.11b/g"
;HKR,Ndi\params\WirelessMode\enum, "8", 0, "Auto"
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"

; For PSP XLink mode, 2006.09.04, by shien chang.
;HKR,Ndi\params\PSPXlinkMode,        ParamDesc,  0, %PSP_XLINK_STR%
;HKR,Ndi\params\PSPXlinkMode,        type,       0, "enum"
;HKR,Ndi\params\PSPXlinkMode,        default,    0, "0"
;HKR,Ndi\params\PSPXlinkMode\enum,   "0",        0, "Disable"
;HKR,Ndi\params\PSPXlinkMode\enum,   "1",        0, "Enable"
;HKR,defaults,PSPXlinkMode,0,"0"
;HKR,,PSPXlinkMode,0,"0"

; Preamble mode, 2006.11.30, by shien chang.
HKR,Ndi\params\PreambleMode, ParamDesc, 0, %PREAMBLE_MODE_STR%
HKR,Ndi\params\PreambleMode, type, 0, "enum"
HKR,Ndi\params\PreambleMode, default, 0, "2"
HKR,Ndi\params\PreambleMode\enum, "1", 0, "Long Preamble"
HKR,Ndi\params\PreambleMode\enum, "2", 0, "Auto"
HKR,Ndi\params\PreambleMode\enum, "3", 0, "Short Preamble"
HKR,defaults,PreambleMode, 0, "2"
HKR,,PreambleMode, 0, "2"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""


;*******************************************************************************
; Destination Directory
;*******************************************************************************
[RTL8187.CopyFiles]
RTL8187.sys,,,2

[DestinationDirs]
DefaultDestDir     = 11
RTL8187.CopyFiles		= 12

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksFiles]
RTL8187.sys = 1

[SourceDisksNames]
1=%DISKNAME%,,,

;*******************************************************************************
; Strings
;*******************************************************************************
[Strings]
Realtek 				= "Ovislink.Corp"
SSID_STR				= "SSID"
CHANNEL_STR				= "Channel"
NETWORK_TYPE_STR		= "Network Type"
LED_CONTROL_STR			= "LED Control" 
POWER_SAVE_STR			= "Power Save Mode"
WIFI_IBSS_STR			= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR		= "Rate Adaptive"
QOS_STR					= "QoS"
WMM_APSD			= "WMM APSD"
CCX_RM_STR				= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR	= "CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR		= "Forced Priority"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR		= "Three Wire Programming Mode"
BOARD_TYPE_STR			= "Board Type"
PROTECTION_MODE_STR		= "Protection Mode"
TPC_STR					= "Transmit Power Control"
TPC_POLARITY_STR		= "TPC Polarity Select"
HIGH_POWER_STR			= "High Power Mechanism"
INIT_GAIN_STR			= "Initial Gain State"
CW_MAX_MIN_STR			= "Contention Window"
PSP_XLINK_STR			= "PSP XLink Mode"
WL_MODE_STR			= "Wireless Mode"
PREAMBLE_MODE_STR		= "Preamble Mode"
FRAGTHRESH_STR			= "Fragmentation Threshold"
RTSTHRESH_STR			= "RTS Threshold"
CHANNEL_PLAN_STR		= "Channel Plan"
FORCEDDATARATE_STR		= "Data Rate"

;; Source disk name
DISKNAME					= "AirLive WL1600USB"
RTL8187.DeviceDesc 			= "AirLive WL1600USB"
RTL8187.DeviceDesc.DispName	= "AirLive WL1600USB"
RTL8187.DeviceDesc.Surecom	= "SURECOM EP-9001-g 802.11g 54M WLAN USB Adapter"
RTL8187.DeviceDesc.Sitecom	= "SITECOM WL-168 Wireless Network USB Adapter 54g"
